   Current meters at the USGS Monterey Canyon Project

   The list below contains information about the files in this zip archive.
   The number in each file name is the record's accession number, which
   identifies it uniquely in the OSU Buoy Group's database.  Thus the current
   meter record whose accession number is 1234 can be found in this archive as
   acc01234.str.  The filename extension, str, indicates that the file has the
   Buoy Group's ASCII stranger format.

----------------------------------------------------------------------------
     file       mooring  instr  water   instrument             dates
     name        name    depth  depth      type
----------------------------------------------------------------------------

   acc07699.str   422     746    806       VACM *      04 Aug 93 - 16 Aug 94

   acc07700.str   423     770   1450       VTCT **     04 Aug 93 - 16 Aug 94
   acc07701.str   423    1250   1450       VACM        04 Aug 93 - 16 Aug 94
   acc07702.str   423    1350   1450       VTCT        04 Aug 93 - 16 Aug 94

   acc07703.str   424    1960   2420       VTCT        04 Aug 93 - 17 Aug 94
   acc07704.str   424    2320   2420       VTCT        04 Aug 93 - 17 Aug 94

   acc07705.str   425    1990   2560       VTCT        04 Aug 93 - 17 Aug 94
   acc07706.str   425    2350   2560       VACM        04 Aug 93 - 17 Aug 94

   acc07707.str   426    1612   2837       VACM        04 Aug 93 - 17 Aug 94
   acc07708.str   426    1982   2837       VTCT        04 Aug 93 - 17 Aug 94
   acc07709.str   426    2342   2837       VACM        04 Aug 93 - 17 Aug 94
   acc07710.str   426    2737   2837       VACM        04 Aug 93 - 17 Aug 94

   acc07711.str   427     213   3223       VACM        06 Aug 93 - 19 Aug 94

   acc07712.str   444     175   3223       VACM        22 Aug 94 - 14 May 95
   acc07713.str   444    3213   3223       VTCT        22 Aug 94 - 14 May 95

   acc07955.str   458    3170   3220       VACM        17 May 95 - 16 Aug 96
   acc07956.str   458    3210   3220       VTCT        17 May 95 - 16 Aug 96

   * VACM = EG&G vector-averaging current meter
   ** VTCT = VACM with a transmissometer